DAQUINO DIGIT, Arduino Uno, USB Portable Digital Data Acquisition Module 

Inputs
       SWITCH ON                         Boolean Start/Stop DAQ board command 

       OUT13...OUT8                      Digital Board Outputs

       PORT (COM256 by def.)           String to indicate the Uno port used (from COM1 to COM256)
					Port COM256 is by default
                         

Outputs
        CONNECTED                        Indicates connection status with Daq Board
        IN2...IN7                        Digital Board Inputs
        

This plugin acts as a digital Data Acquisition Module which used the well-known Arduino UNO Platform

CReSTIC 2021. All rights reserved.