DAQUINO DIGIT ANALOG. Arduino Uno, USB Portable Digital & Analog Data Acquisition Module 

Inputs
        SWITCH ON  			Boolean Start/Stop DAQ board command 

        OUT13...OUT11			Digital Board Outputs
	OUT8

	OUT10, OUT9 (PWM)		PWM analog representation of byte value (from 0 to 255)

	PORT (COM256 by def.)          String to indicate the Uno port used (from COM1 to COM256)
					Port COM256 is by default
                         

Outputs
        CONNECTED                       Indicates connection status with Daq Board 
        A0...A2                         (Byte) Analog Board Inputs
        IN2...IN7                       (Boolean) Digital Board Inputs


This plugin acts as a digital and Analog Data Acquisition Module which used the well-known Arduino UNO Platform


CReSTIC 2021. All rights reserved.